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October 20, 2026

Brian L. Pearl 
Deputy Director
United States Government Publishing Office
732 North Capitol Street NW
Washington DC 20401

RE:	Permit No. 7450 to Construct and Operate a Canon ProStream 2000 Series Industrial Web-fed Inkjet Printer (Press Group 55 / Unit ID 5591)


Dear Brian L. Pearl:

Pursuant to sections 200.1 and 200.2 of Title 20 of the District of Columbia Municipal Regulations (20 DCMR), a permit from the Department of Energy and Environment (“the Department”) shall be obtained before any person can construct and operate a new stationary source in the District of Columbia. The application of United States Government Publishing Office (GPO) (“The Permittee”) to construct and operate a new Canon ProStream 2000 Series industrial web-fed inkjet printer (Press Group 55 / Unit ID 5591) on the fourth floor of Building C, at 732 North Capitol Street NW, Washington DC 20401, per the submitted plans and specifications received by the Department on May 22, 2026, is hereby approved, subject to the following conditions: 

I.	General Requirements:

a. The Canon ProStream 2000 Series Industrial Web-fed Inkjet digital Printer shall be constructed and operated in compliance with the applicable air pollution control requirements of 20 DCMR.

b.	This permit expires on October 19, 2031 [20 DCMR 200.4]. If continued operation after this date is desired, the Permittee shall submit a request for an extension by June 19, 2031.

c. Construction or operation of equipment under the authority of this permit shall be considered acceptance of its terms and conditions.

d. The Permittee shall allow authorized officials of the District, upon presentation of identification, to: 

1.	Enter upon the Permittee’s premises where a source or emission unit is located, an emissions related activity is conducted, or where records required by this permit are kept;
2.	Have access to and copy, at reasonable times, any records that must be kept under the terms and conditions of this permit; 

3.	Inspect, at reasonable times, any facilities, equipment (including monitoring and air pollution control equipment), practices, or operations regulated or required under this permit; and

4.	Sample or monitor, at reasonable times, any substance or parameter for the purpose of assuring compliance with this permit or any applicable requirement.

e.	This permit shall be kept on the premises and produced upon request.

f.	Failure to comply with the provisions of this permit may be grounds for suspension or                                                                                          revocation. [20 DCMR 202.2]

g.	Within twelve (12) months of initial startup of the printer, the Permittee shall submit a complete application (or application revision, if another application to renew or modify the permit is already pending) to modify the facility’s Title V operating permit to incorporate the requirements of this permit in that Title V operating permit. [20 DCMR 301.1(a)(2)]. For purposes of this condition and Condition VI(d), “startup” means the setting in operation of the source or portion of the source for any purpose.

II.	Emission Limitations:
	
a. Volatile organic compound (VOC) emissions from this equipment shall not exceed 0.61 tons in any 12-consecutive-month rolling period. [20 DCMR 201]

b. No person shall discharge into the atmosphere more than fifteen (15) pounds of VOC emissions in any one (1) day, nor more than three pounds (3 lb.) in any one (1) hour, from any combination of articles, machines, units, equipment, or other contrivances at a facility, unless the uncontrolled VOC emissions are reduced by at least ninety percent (90%) overall capture and control efficiency. [20 DCMR 700.2]

c.	No visible emissions shall be emitted from this equipment. [20 DCMR 201 and 20 DCMR 606.1(a)(2)]

d.	An emission into the atmosphere of odorous or other air pollutants from any source in any quantity and of any characteristic, and duration which is, or is likely to be injurious to the public health or welfare, or which interferes with the reasonable enjoyment of life or property is prohibited. [20 DCMR 903.1]  

Violation of the requirements of this condition that occur as a result of unavoidable malfunction, despite the conscientious employment of control practices, shall be an affirmative defense for which the owner or operator shall bear the burden of proof. A malfunction shall not be considered unavoidable if the owner or operator could have taken, but did not take, appropriate steps to eliminate the malfunction within a reasonable time, as determined by the Department. [20 DCMR 903.13(b)]

Note: This condition is District enforceable only.

III.	Operational Limitations:

a.	The Permittee shall not use more than the following quantities of materials on the printer in any 12-consecutive-month period. Any other materials used on the printer shall not contain volatile organic compounds (VOCs).

1.	85,147 lbs. of each of the following inks:

i.	ProStream Ink Black KP70;

ii.	ProStream Ink Cyan CP72; 

iii.	ProStream Ink Magenta MP70;

iv.	ProStream Ink Yellow YP70; and

2.	1.5 gallons of SU90 cleaning solvent. 

b. At all times, including periods of startup, shutdown, and malfunction, the Permittee shall, to the extent practicable, maintain and operate the unit in a manner consistent with good air pollution control practice for minimizing emissions. Determination of whether acceptable operating procedures are being used will be based on information available to the Department which may include, but is not limited to monitoring results, opacity observations, review of operating and maintenance procedures, and inspection of the source. [20 DCMR 201 and 20 DCMR 606.4(a)]

c.	The Permittee shall maintain all of the equipment covered by this permit in accordance with one of the following [20 DCMR 606.4(b)]

1. The manufacturer’s emission-related written instructions; or

1. Unless preempted by specific federal regulation, an alternate written maintenance plan approved in writing by the Department.

d.	The Permittee shall ensure that persons participating in the maintenance and operation of equipment are adequately trained and supervised to meet the requirements of Conditions III(b) and (c). [20 DCMR 606.4(c)]

IV.	Monitoring and Testing Requirements:

a.	The Permittee shall conduct and allow the Department access to conduct tests of air pollution emissions from any source as requested [20 DCMR 502.1].

b.	The Permittee shall monitor the identities, VOC contents, and quantities of each VOC-containing material used on the equipment covered by this permit so as to ensure compliance with Condition III(a).

c. Unless a specific method is specified elsewhere in this permit, the VOC content of a substance shall be determined based on the Safety Data Sheet (SDS) of the material, EPA Reference Method 24, or any other method approved in advance by the Department.

d. The Permittee shall monitor the emission points from the printing press to ensure that the requirements of Condition II(c) are met.

e. The Permittee shall maintain an awareness of the area to ensure that the odor and nuisance air pollutant requirements of Condition II(d) are met.

V.	Record Keeping Requirements:

a.	The Permittee shall maintain records of the information specified in Condition V(b) in a readily accessible location at the facility, or an electronic location readily accessible from the facility, for a minimum of five (5) years from the date each record is recorded and shall make these records available to the Department and EPA upon written or verbal request. [20 DCMR 104.2(b), 20 DCMR 302.1(c)(2)(B), 20 DCMR 500.1, 20 DCMR 500.8, and 20 DCMR 606.5(d)] All records shall be maintained in such a manner that authorized representatives can certify their accuracy under penalty of D.C. Official Code § 8-101.05e pertaining to false statements, and have either done so in the records, or will do so upon request at the time they are made available to the Department or EPA. [20 DCMR 104.2 and 20 DCMR 500.1]

1.	The records shall provide sufficient data and calculations to demonstrate clearly that the emission limitations or control requirements are met; and

2.	Data or information required to determine compliance with an applicable limitation shall be recorded and maintained in a time frame consistent with the averaging period of the standard.

b.	The Permittee shall maintain the following records in accordance with Condition V(a):

1.	Records of the identity and VOC content of each ink, cleaning solution, or other VOC-containing material used in conjunction with the equipment each month;

2.	Records of the quantity of each VOC-containing material used on the printer each month;

3.	Records of the total pounds of all inks used by the printer, maintained in a 12-month rolling sum format, updated monthly, to document compliance with Condition III(a);

4. Records of the total 12-month rolling VOC emissions from the equipment, updated   monthly;

5. Records of all maintenance performed on the printer;

6. Records of any complaints or exceedances related to the odor requirements of Condition II(d) and the response taken by the Permittee to investigate and correct any identified problems(s); and

7. Records of any deviations from the requirements of Conditions II and III of this permit.

c.	For any malfunction, the Permittee shall investigate the cause of the malfunction and maintain records of the investigatory activities and conclusions of such investigation [20 DCMR 606.5]:

d.	The Permittee shall maintain records of personnel training related to maintenance and operation of the equipment to document compliance with Condition III(d).


VI.	Reporting Requirements [20 DCMR 200.8]:

a.	The Permittee shall furnish to the Department, upon receipt of a written request and within a reasonable time, any information that the Department may request to determine whether cause exists for, reopening, or revoking the permit or to determine compliance with the permit. Upon request, the Permittee shall also furnish to the Department copies of records required to be kept by the permit. [20 DCMR 104.2(b) and 20 DCMR 302.1(g)(5)]

b.	The Permittee shall comply with the reporting requirements of Condition I(d) of Chapter 3 permit 029-R1-A4 for the equipment covered by this permit, including incorporating the conditions of this permit in each semi-annual and annual compliance certification submitted to the Department, except that:

1.	For any threat to public health, safety, and the environment, the Permittee shall immediately report any permit deviation that poses an imminent and substantial danger to public health, safety, or the environment to the following (in order): [20 DCMR 104.2(b) and 20 DCMR 302.1(c)(3)(C)(ii)] 

i.	Dial 911. DC Fire and Emergency Medical Services (FEMS) is the District’s first response agency for hazardous materials releases;

ii.	Call the National Response Center at (800) 424-8802;

iii.	Contact the District’s Homeland Security and Emergency Management Agency at (202) 727-6161.

For more information on reporting emergencies, see the DOEE Environmental Emergency Management Program website at: https://doee.dc.gov/service/environmental-emergency-management-program-eemp; and

2.	Rather than reporting emissions exceedances to the Department’s Emergency Operations Number listed in Permit 029-R1-A4, Condition I(d)(4)(C), such emissions exceedances shall be reported to air.quality@dc.gov. 

c.	The Permittee shall, within 15 days of initial “startup” of the printer (see Condition I(g)), notify the Department in writing of the date of the unit’s startup.

d.	All reports required pursuant to this permit shall be submitted electronically to air.quality@dc.gov, except where additional reporting requirements are specified in Condition I(d) of Chapter 3 Permit 029-R1-A4.

If you have any questions, please contact me at (202) 498-8143 or stephen.ours@dc.gov or Afewerki Birhane at (202) 573-5029 or afewerki.birhane@dc.gov.

Sincerely,



Stephen S. Ours, P.E.
Chief, Permitting Branch
Air Quality Division
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